#Feedback Loop Configuration File
#
#Each line of this file defines a configuration slot and consists of integer numbers delimited by white 
#spaces in the following order:
#ADDSUB_MODE ADD_INPUT_MUX DELAY FACTOR TIMESTAMP
#
#ADDSUB_MODE:   Select feedback mode (0=negative, 1=positive)
#ADD_INPUT_MUX: Select feedback input (0=GND[only ADC Input 1], 1=ADC Input 2[Both ADC inputs are used])
#DELAY:         Clock cycles counts (50 ns period) to delay the feedback signal [0-255]
#FACTOR:        Multiplication factor to apply to the feedback signal [0-16] (NOTE: Integer is intepreted as a 1Q4 Fixed Point Number!)
#TIMESTAMP:     Defines the clock count number from the sync pulse from which on the configurations settings will be applied. [32-bit unsigned integer] 
#               First Config slot should have a timestamp equal to zero.
1   0   0   8   0
0   0   0   8   1200000000
