onerror {resume}
quietly WaveActivateNextPane {} 0
add wave -noupdate -divider SYSTEM
add wave -noupdate /l1_rtps_writer_test1/uut/clk
add wave -noupdate /l1_rtps_writer_test1/uut/reset
add wave -noupdate -radix unsigned /l1_rtps_writer_test1/uut/time
add wave -noupdate -radix unsigned /l1_rtps_writer_test1/uut/check_time
add wave -noupdate -divider INPUT
add wave -noupdate -group META /l1_rtps_writer_test1/uut/empty_meta
add wave -noupdate -group META /l1_rtps_writer_test1/uut/rd_meta
add wave -noupdate -group META /l1_rtps_writer_test1/uut/last_word_in_meta
add wave -noupdate -group META -radix hexadecimal /l1_rtps_writer_test1/uut/data_in_meta
add wave -noupdate -expand -group USER /l1_rtps_writer_test1/uut/empty_user
add wave -noupdate -expand -group USER /l1_rtps_writer_test1/uut/rd_user
add wave -noupdate -expand -group USER -radix hexadecimal /l1_rtps_writer_test1/uut/data_in_user
add wave -noupdate -expand -group USER /l1_rtps_writer_test1/uut/last_word_in_user
add wave -noupdate -divider HC
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/data_available
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/start_hc
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/opcode_hc
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/ack_hc
add wave -noupdate -group HC -radix unsigned /l1_rtps_writer_test1/uut/seq_nr_hc
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/done_hc
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/ret_hc
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/get_data_hc
add wave -noupdate -group HC -radix hexadecimal /l1_rtps_writer_test1/uut/data_in_hc
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/valid_in_hc
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/ready_in_hc
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/last_word_in_hc
add wave -noupdate -group HC -radix hexadecimal /l1_rtps_writer_test1/uut/cc_instance_handle
add wave -noupdate -group HC /l1_rtps_writer_test1/uut/cc_kind
add wave -noupdate -group HC -radix unsigned /l1_rtps_writer_test1/uut/cc_source_timestamp
add wave -noupdate -group HC -radix unsigned /l1_rtps_writer_test1/uut/cc_seq_nr
add wave -noupdate -divider OUTPUT
add wave -noupdate -expand -group OUTPUT /l1_rtps_writer_test1/uut/full_ro
add wave -noupdate -expand -group OUTPUT /l1_rtps_writer_test1/uut/wr_ro
add wave -noupdate -expand -group OUTPUT -radix hexadecimal /l1_rtps_writer_test1/uut/data_out_ro
add wave -noupdate -expand -group OUTPUT /l1_rtps_writer_test1/uut/last_word_out_ro
add wave -noupdate /l1_rtps_writer_test1/rtps_out_inst/wr
add wave -noupdate -radix hexadecimal /l1_rtps_writer_test1/rtps_out_inst/data_out
add wave -noupdate -divider {MAIN FSM}
add wave -noupdate /l1_rtps_writer_test1/uut/stage
add wave -noupdate /l1_rtps_writer_test1/uut/cnt
add wave -noupdate /l1_rtps_writer_test1/uut/w_map
add wave -noupdate /l1_rtps_writer_test1/uut/ind
add wave -noupdate -radix unsigned /l1_rtps_writer_test1/uut/last_seq_nr
add wave -noupdate -radix unsigned /l1_rtps_writer_test1/uut/global_ack_seq_nr_base
add wave -noupdate -radix unsigned /l1_rtps_writer_test1/uut/next_seq_nr
add wave -noupdate -divider {MEMORY FSM}
add wave -noupdate /l1_rtps_writer_test1/uut/mem_op_done
add wave -noupdate /l1_rtps_writer_test1/uut/mem_op_start
add wave -noupdate /l1_rtps_writer_test1/uut/mem_opcode
add wave -noupdate /l1_rtps_writer_test1/uut/mem_stage
add wave -noupdate /l1_rtps_writer_test1/uut/mem_cnt
add wave -noupdate -radix unsigned -childformat {{/l1_rtps_writer_test1/uut/mem_addr_base(6) -radix unsigned} {/l1_rtps_writer_test1/uut/mem_addr_base(5) -radix unsigned} {/l1_rtps_writer_test1/uut/mem_addr_base(4) -radix unsigned} {/l1_rtps_writer_test1/uut/mem_addr_base(3) -radix unsigned} {/l1_rtps_writer_test1/uut/mem_addr_base(2) -radix unsigned} {/l1_rtps_writer_test1/uut/mem_addr_base(1) -radix unsigned} {/l1_rtps_writer_test1/uut/mem_addr_base(0) -radix unsigned}} -subitemconfig {/l1_rtps_writer_test1/uut/mem_addr_base(6) {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_addr_base(5) {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_addr_base(4) {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_addr_base(3) {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_addr_base(2) {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_addr_base(1) {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_addr_base(0) {-height 15 -radix unsigned}} /l1_rtps_writer_test1/uut/mem_addr_base
add wave -noupdate -childformat {{/l1_rtps_writer_test1/uut/mem_endpoint_data.addr -radix unsigned} {/l1_rtps_writer_test1/uut/mem_endpoint_data.guid -radix hexadecimal} {/l1_rtps_writer_test1/uut/mem_endpoint_data.ip_addr -radix hexadecimal} {/l1_rtps_writer_test1/uut/mem_endpoint_data.portn -radix hexadecimal} {/l1_rtps_writer_test1/uut/mem_endpoint_data.lease_deadline -radix hexadecimal} {/l1_rtps_writer_test1/uut/mem_endpoint_data.res_time -radix unsigned} {/l1_rtps_writer_test1/uut/mem_endpoint_data.ack_seq_nr_base -radix unsigned} {/l1_rtps_writer_test1/uut/mem_endpoint_data.req_seq_nr_base -radix unsigned}} -expand -subitemconfig {/l1_rtps_writer_test1/uut/mem_endpoint_data.addr {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_endpoint_data.guid {-height 15 -radix hexadecimal} /l1_rtps_writer_test1/uut/mem_endpoint_data.ip_addr {-radix hexadecimal} /l1_rtps_writer_test1/uut/mem_endpoint_data.portn {-height 15 -radix hexadecimal} /l1_rtps_writer_test1/uut/mem_endpoint_data.lease_deadline {-height 15 -radix hexadecimal} /l1_rtps_writer_test1/uut/mem_endpoint_data.res_time {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_endpoint_data.ack_seq_nr_base {-height 15 -radix unsigned} /l1_rtps_writer_test1/uut/mem_endpoint_data.req_seq_nr_base {-height 15 -radix unsigned}} /l1_rtps_writer_test1/uut/mem_endpoint_data
add wave -noupdate -group MEM_CTRL -radix unsigned /l1_rtps_writer_test1/uut/mem_addr
add wave -noupdate -group MEM_CTRL /l1_rtps_writer_test1/uut/mem_valid_in
add wave -noupdate -group MEM_CTRL /l1_rtps_writer_test1/uut/mem_ready_in
add wave -noupdate -group MEM_CTRL /l1_rtps_writer_test1/uut/mem_read
add wave -noupdate -group MEM_CTRL -radix hexadecimal /l1_rtps_writer_test1/uut/mem_write_data
add wave -noupdate -group MEM_CTRL /l1_rtps_writer_test1/uut/abort_read
add wave -noupdate -group MEM_CTRL /l1_rtps_writer_test1/uut/mem_valid_out
add wave -noupdate -group MEM_CTRL /l1_rtps_writer_test1/uut/mem_ready_out
add wave -noupdate -group MEM_CTRL -radix hexadecimal /l1_rtps_writer_test1/uut/mem_read_data
add wave -noupdate -divider TESTBENCH
add wave -noupdate -group TESTBENCH /l1_rtps_writer_test1/start_meta
add wave -noupdate -group TESTBENCH /l1_rtps_writer_test1/packet_sent_meta
add wave -noupdate -group TESTBENCH /l1_rtps_writer_test1/start_user
add wave -noupdate -group TESTBENCH /l1_rtps_writer_test1/packet_sent_user
add wave -noupdate -group TESTBENCH /l1_rtps_writer_test1/stage_hc
add wave -noupdate -group TESTBENCH /l1_rtps_writer_test1/out_check_done
add wave -noupdate -group TESTBENCH /l1_rtps_writer_test1/stim_done
add wave -noupdate -group TESTBENCH /l1_rtps_writer_test1/test_done
add wave -noupdate -divider MISC
add wave -noupdate /l1_rtps_writer_test1/uut/req_bitmap_pos
add wave -noupdate /l1_rtps_writer_test1/uut/req_seq_nr_bitmap
add wave -noupdate /l1_rtps_writer_test1/uut/nack_bitmap_pos
add wave -noupdate /l1_rtps_writer_test1/uut/bitmap_latch
TreeUpdate [SetDefaultTree]
WaveRestoreCursors {Cursor {32325000 ps} 1} {{Cursor 4} {35075000 ps} 1} {{Cursor 5} {32315215 ps} 0}
quietly wave cursor active 3
configure wave -namecolwidth 150
configure wave -valuecolwidth 135
configure wave -justifyvalue left
configure wave -signalnamewidth 1
configure wave -snapdistance 10
configure wave -datasetprefix 0
configure wave -rowmargin 4
configure wave -childrowmargin 2
configure wave -gridoffset 0
configure wave -gridperiod 1
configure wave -griddelta 40
configure wave -timeline 0
configure wave -timelineunits ns
update
WaveRestoreZoom {30922320 ps} {31924224 ps}
