# This message communicates ROS Time defined here:
# https://design.ros2.org/articles/clock_and_time.html

# The seconds component, valid over all int32 values.
int32 sec

# The nanoseconds component, valid in the range [0, 10e9).
uint32 nanosec
